Last Modified: 1/13/96

Daedalus Glossary

Table 1:

Base Station This is the connection between the wired and wireless networks.

External Base Station An External Base Station is one that we has no control over in terms of modifying code running on the base station. Examples are CDPD and Metricom (in some cases).

External Controller This as a mechanism that allows the user (to handle exceptional conditions) or Proxy (in the case of load balancing) to provide advice to the Handoff Controller in its choice of network or base station.

Handoff Controller This component handles the transition when a mobile device moves from one base station to another (horizontal handoff) or when a mobile deice moves from one network to another (vertical handoff). It sends the encapsulation/decapusation requests to base stations. It makes all handoff decisions due to mobility by listening to beacon packets sent by the base stations.

Horizontal Handoff This occurs when a mobile device moves between base stations of the same network.

Internal Base Station An Internal Base Station is one that we have control over in terms of modifying code running on the base station. Examples are Wavelan and Metricom (in some cases).

Network Monitor This component makes all measurements having to do with network interfaces. This component does the statistical modeling of each network interface, and collects statistics having to do with the quality of the connections between the Proxy and the mobile over each wireless network.

Vertical Handoff This occurs when a mobile device moves from a base stations of one network to a base station of a different network.